**XYZ THERMAX 6 DUO, CPU Air Cooler, 6 Direct Heat pipe,Dual Tower, 2x Vortex 120mm A-RGB fan**

**Introducing the XYZ Thermax 6 DUO A-RGB. Our ideal air cooling solution to keep your processor at optimal temperatures, even during the most demanding tasks. Its dual fan design with customizable ARGB lighting, 6 heat pipes per side, and its wide socket compatibility make it the perfect choice for gamers and PC enthusiasts.**

**Key Features:**

1. **Efficient Cooling:** Maximize heat dissipation with twelve high-quality copper heat pipes (six per tower), ensuring optimal performance at all times.
2. **Dual Fan Configuration:** Experience powerful airflow with two high-performance Vortex A-RGB fans operating at 600-2000 RPM, providing 62.7 CFM each with minimal noise of only 18.4dB(A).
3. **Vibrant ARGB Lighting:** Customize and create stunning lighting effects with the integrated ARGB LEDs, adding a touch of style to your PC.
4. **Durable Build and Easy Installation:** Enjoy long-lasting and quiet operation thanks to fluid dynamic bearings and a hassle-free installation process.
5. **Wide Socket Compatibility:** Versatile cooling for your system with compatibility for a wide range of sockets, including AMD: FM AM3 AM4 AM5 / Intel: LGA 115X/1366/2011/1700/1200/1851
6. **Optimized Design:** Maximize airflow and cooling efficiency with the heatsink's optimized design, keeping your CPU running at optimal temperatures even during the most demanding tasks.

**Technical Specifications:**

**Thermax 6 DUO ARGB Heatsink:**

* **Socket Compatibility:** AMD: FM AM3 AM4 AM5 / Intel: LGA 115X/1366/2011/1700/1200/1851
* **Fan Configuration:** 2 fans, 0.28A 12VDC, 600-2000 RPM, 62.7 CFM, 33 dB(A) MAX, 18.5dB(A) MIN
* **LED Mode:** ARGB
* **Heatpipes:** 6 copper heatpipes per tower (12 total)
* **Bearing Type:** Fluid dynamic bearing
* **Fan Size:** 120 mm x 120 mm x 25 mm
* **Overall Heatsink Size:** 154 mm x 132 mm x 125 mm

**Vortex A-RGB Fan:**

* **Model and Dimensions:** Vortex A-RGB, 120x120x25 mm
* **Rated Voltage:** DC 12V
* **Operating Voltage Range:** 10.8~13.2V
* **Starting Voltage:** DC 5V MAX (Rated Voltage, 25℃, 65% RH)
* **Rated Current:** 0.15A±20%
* **Locked Current:** 0.20A±20%
* **Power Consumption:** 1.8W±20%
* **Speed:** 600-2000±10% RPM (Rated Voltage, 25℃, 65% RH, Free Air)
* **Max. Airflow:** 62.7 CFM
* **Max. Static Pressure:** 2.68 mm-H₂O
* **Max Noise Level (2000rpm):** 32 dB(A)
* **Min Noise Level (600rpm):** 18.5 dB (A)
* **Lifespan:** 60,000 hours at 25℃ (MTBF Confidence Level 90%)
* **ARGB Connector:** ARGB Head, Female to Male

**Avaliable Colors:**

**White**

SKU | X-AC-THERDUOW6

EAN | 6978262010805

**Black**

SKU | X-AC-THERDUOB6

EAN | 6978262010799