**XYZ AQUAPULSE FUSION 360 AIO Liquid CPU Cooler, A-RGB Tubes Design, Digital Temp Screen, 3x Pulsar 120mm PWM A-RGB Fans**

**Master the heat and take your performance to the next level with the XYZ AQUAPULSE FUSION 360 AIO Liquid CPU Cooler. This all-in-one liquid cooling solution combines exceptional performance, captivating ARGB aesthetics, and intelligent features to keep your CPU running at optimal temperatures, even under the most demanding workloads.**

**Key Features:**

1. **ARGB Tubes Design:** Take lighting to another level with the integrated ARGB tubes in the AQUAPULSE FUSION 360. Create a fluid and dynamic light show that runs throughout the cooling system, adding a unique touch of style to your PC.
2. **Digital Temperature Screen:** Maintain precise control over your CPU temperature with the digital display integrated into the pump block. Monitor your system's performance in real-time and adjust settings as needed.
3. **Three 120mm PWM Pulsar A-RGB Fans:** Enjoy quiet and efficient cooling with the three included 120mm Pulsar fans. These PWM fans offer precise speed control and feature customizable ARGB lighting to complement the light show of the tubes.
4. **Easy Installation:** AQUAPULSE FUSION 360 is designed for simple and hassle-free installation, with a universal mounting bracket compatible with a wide range of Intel and AMD sockets.
5. **High-Efficiency Pump:** The high-efficiency pump ensures a constant flow of coolant, maximizing heat dissipation and keeping your CPU running at optimal temperatures even under heavy workloads.

**Technical Specifications:**

**General Specifications:**

* **Rated Voltage:** 12V DC
* **Minimum Starting Voltage:** ≤4.0 V
* **Electric Current:** ≈0.30 A
* **Power:** ≤3.6 W
* **Maximum Head:** 1.5M
* **Minimum Flow Rate:** ≥1300 mL/min
* **Speed:** 2500RPM±10%
* **Storage Temperature:** -10°C ~ 70°C
* **Operating Temperature:** -10°C ~ 60°C
* **Longest Service Life:** 50000 hours under normal working conditions
* **Maximum Noise:** ≤30 db
* **Pump Size:** L67.6W82.3H55.5mm
* **Catheter:** Braided tube L=380 ± 2mm with ARGB lighting
* **Dimension:** L397W120H27mm
* TDP: 340W
* **Socket Support:**
  + Intel: LGA 115X/1366/2011/1700/1200/1851
  + AMD: AM5/AM4
* **ARGB Connector:** Included for motherboard synchronization
* **TDP:** 340W

**Technical Specifications - Pulsar 120mm PWM A-RGB Fans**

* **Model:** PULSAR
* **Outside Dimensions:** 120 x 120 x 25 mm
* **Bearing Type:** Rifle Bearing
* **Voltage:**
  + Rated Voltage: DC 12V
  + Operating Voltage: 10.8 ~ 13.2V
  + Starting Voltage: DC 5V MAX
* **Current:**
  + Rated Current: 0.28A ±10% MAX
  + Tag Current: 0.28A ±10% MAX
  + Blocking Current: 0.30A ±10% MAX
* **Power Consumption:** 3.36W ±10% MAX
* **Rotation Speed:** 600-1800 ±10% RPM
* **Maximum Air Flow:** 78.64 CFM (ft³/min)
* **Max. Static Pressure:** 1.78mm-H₂O
* **Max. Noise Level:** 36dB(A)
* **Min. Noise Level:** 18.5dB(A)
* **Lifetime:** 50,000 hours at 25°C
* **Number of Blades:** 9
* **Number of Poles:** 4
* **ARGB Connector:** Included for motherboard synchronization

**Avaliable Colors:**

**White**

SKU | X-WC-AQUA-FU-360W

EAN | 6978262010423

**Black**

SKU | X-WC-AQUA-FU-360B

EAN | 6978262010409